### Constructing a Plane from an Alignment

A plane can be constructed through the current origin and parallel to the current work plane. (Input features do not need to be provided.)

To construct an alignment plane:

1. Access the Construct Plane dialog box (Insert | Feature | Constructed | Plane).

2. Select the Alignment option.

3. Do not select any features.

4. Click the Create button.

The Edit window command line for this option would read: CONSTR/PLANE,ALIGN

Constructing a Plane from an Alignment | A - Plane constructed parallel to the top (XY+Z) work plane and through the origin. B - Origin (0,0,0) C - Current work plane