### Level

The Level button allows you to establish the orientation of the normal axis of the current working plane.

To choose a feature to "level" to:

1. Select the feature to be used from the Feature List box.

2. Click the Level button.

The Level button only becomes active if you first select a feature from the feature list or an existing level sub-command (ALIGNMENT/LEVEL). If you select an existing level sub-command, it will be modified to use the new feature selection; otherwise a new level sub-command will be created using the selected feature.

You may also specify the axis to be used in establishing the orientation by selecting it from the drop-down list.

The Edit window command line for this option reads:
ALIGNMENT/LEVEL,ZPLUS,'feat_id'

Changeable fields:
"ZPLUS"
This is a field that allows you to switch between the fields ZPLUS, XPLUS, YPLUS, ZMINUS, XMINUS, and YMINUS in the Edit window. This field represents the direction of the specified axis that the feature is leveled to.

"feat_id"
The alignment levels to the specified feature.
Example: PLANE1.