#### Deviation Symbols

The Deviation Symbols check box shows the deviation within the set range. If the out of tolerance range is high, PC-DMIS will indicate the deviation using the "greater than" symbol (>) on the right side of the line. If the out of tolerance range is low, PC-DMIS will indicate the deviation using the "less than" symbol (<).

For example:
Nominal = 0.00
Measured = 0.02
Positive Tolerance = 0.10
Negative Tolerance = 0.20
Total Tolerance Range = (.10 - (-.20)) = .30
Percentage = 100*(.02 - (-.20))/.3 = 73.3 %
- - - - - - # - - looks at the % and shifts based on the %.

DIM D1= LOCATION OF CIR F5 GRAPH=OFF TEXT=OFF MULT=1.00

AX | NOM | +TOL | -TOL | MEAS | DEV | OUT-TOL |
x | 5.0000 | 0.0100 | 0.0100 | 5.0000 | 0.0000 | 0.0000 | ----#----
y | 2.0000 | 0.0100 | 0.0100 | 2.0000 | 0.0000 | 0.0000 | ----#----
z | -0.2500 | 0.0100 | 0.0100 | -0.2500 | 0.0000 | 0.0000 | ----#----
d | 2.0000 | 0.0100 | 0.0100 | 2.0000 | 0.0000 | 0.0000 |
v | i | j | k |  |  |  |

END OF DIMENSION D1