#### Step 2: Install OrbixE2A on the PC-DMIS PC

1. Insert disc 1 of the I-DEAS installation discs in the PC-DMIS PC.

2. Select installation for I-DEAS 10 NX Series. For I-DEAS versions later than 10, the version number will change.

3. Follow any on-screen instructions until the Setup Type dialog box appears.

4. At the Setup Type dialog box, select Software Installation Only.

5. At the User Information dialog box, type the same installation number that you used to install I-DEAS on the remote computer.

6. At the Select License File dialog box, select Manually configure my license after setup completes.

7. At the Select Components dialog box, select the A001 Core Master Modeler check box. Leave all other options deselected.

8. Finish the installation process by following any additional on-screen instructions.