Current Help System: PC-DMIS Fixturing (View Core Help)

#### Five NT

Five NT dialog box

The Five NT dialog box allows you to specify the files that define the System V (DCC) fixturing files that you want to import. Follow these steps to import fixturing files:

1. Select the File | Import | Five NT menu option to import DCC fixturing system data.

2. Browse to the Directory of old Five NT Files to import to specify the path of the Five NT file that you want to import.

3. Browse to the Directory of COSTAN.dat for Five NT to specify the location of the COSTAN,dat file to be used with Five NT.

4. Select the need file(s) from the Existing Five NT files list box. This list box displays the available files to import the need DCC fixturing systems.

5. Click the Import button to import the selected files.

The imported system is now ready to be configured and used with PC-DMIS.