Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Curve Type

This option determines the type of curve for your spline path. An open curve passes through the start, control, and end points and then stops. A closed curve does the same but when the curve passes through the end point, it also returns to the start point.

Entry Name: ScanDialogClrPln

Entry Type: Whole Number specifying Open (1) or Closed (0). Default value is 1.