Current Help System: PC-DMIS Settings Editor (View Core Help)

### Low Threshold (0-3)

The Low Threshold values provide an lower limit (in the appropriate units) on the current temperature below which no further thermal compensation will be applied.

Entry Name: LowThreshold(0-3)

Entry Type: Character String specifying degrees in either Celsius or Fahrenheit. Default value is 0.0.

Number Key:

0 | X Axis
1 | Y Axis
2 | Z Axis
3 | Part