Current Help System: PC-DMIS Settings Editor (View Core Help)

### Prior Temp (0-31)

These values store the previous readings from your temperature sensors for your slave arm. You can have anywhere from 1 to 32 sensors. These values are provided in Celsius or Fahrenheit according to the TempCompCelsius value.

Entry Name: PriorTemp(0-31)

Entry Type: Character String to specify temperature. Default value is 0.0.