Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Perm Hits

Allows you to define the default value for the Perm Hits option that will be used when an Auto Feature is created. The Perm Hits value allows you to select the number of sample hits taken for the auto feature. These hits are used to measure the plane around the nominal point location. Perm sample hits are taken all subsequent measurements during execution of the part program after the initial measurement.

Entry Name: DccPermHits

Entry Type: Whole Number to specify the number of Perm hits. Default value is 0.

See the "Hit Controls area" topic for information on valid values and proper use of initial and permanent hits.