Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Ring Dont Update Tip Diameter

When this value is set to TRUE (1), the contact probe tip diameter will not be updated based on the measurements taken with the ring tool. You want this value to be TRUE (1) when a sphere tool is being used for tip diameter calibration instead of a ring.

Entry Name: ProbeQualRingDontUpdateTipDiameter

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.