Current Help System: PC-DMIS Settings Editor (View Core Help)

### TC Final Adjust Height (toolchanger)

This offset value provides the height distance that is applied to a calibrated port location of various toolchangers, specified in the Toolchangers list below. This adjusts the port location up or down relative to the toolchanger if you are directly in front of it.

- If a negative value is used, the calibrated port location is adjusted up relative to the toolchanger's Z axis by the given distance.

- If a positive value is used, the calibrated port location is adjusted down relative to the toolchanger's Z axis by the given distance.

Note: Since toolchangers can be placed on the machine in varying orientations with respect to the machine's axes, adjustments made to the calibration are relevant to the toolchanger's own coordinates and not the machine's axes.

Entry Name: TCFinalAdjustHeight(toolchanger)

Entry Type: Real Number specifying height adjustment distance. Default value is 0.

Toolchangers

- FCR25SM25

- FCR25TM25

- PMM

- SCP600

- SCP80

- SP600

- TESASTAR-PR

- TP20

- TP200