Current Help System: PC-DMIS Settings Editor (View Core Help)

### Use Legacy Slot Vector

This entry lets you specify the vector PC-DMIS will use when constructing an Intersect Point or Drop Point if one of the inputs is a slot. When this entry is set to TRUE (1), PC-DMIS will use the slot normal vector. When this entry is set to 0, PC-DMIS will use the slot centerline vector.

Entry Name: UseLegacySlotVector

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.