Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto LIV Freeze

With this value set to TRUE, this will cause the Live View Freeze button to be automatically pressed on and off at program execution time, so that measured points are frozen on the screen until the next points are measured. This is also useful for machines where “image tear” occurs during stage movements.

Entry Name: AutoLIVFreeze

Entry Type: True/False value. Default value is FALSE.