Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC H Pnt Tol

Allows you to define the default value for the Tolerance option that will be used when an Auto High Point is created. Allows you to define High Point tolerance that PC-DMIS will use to stop searching for a high point within a given area. The tolerance value should always be less than the increment value. During the search process, PC-DMIS decreases the increment value until it is less than or equal to the Tolerance value supplied, indicating that the highest point in the current work plane has been located.

Entry Name: DccHPntTol

Entry Type: Real Number to specifying distance. Default value is 0.