Current Help System: PC-DMIS Settings Editor (View Core Help)

### Mode

This option determines which mode your computer will use in a Multiple Arm Setup

Entry Name: Mode

Entry Type: Whole Number specifying mode. Default value is -1.

Mode Key:

0 | This computer (slave) relays commands from main computer
1 | This computer (master) drives all arms
2 | This computer is not used in a multiple arm setting