Current Help System: PC-DMIS Settings Editor (View Core Help)

### Ring Band_Inner

Provides the offset from the theoretical feature radius or form for the inner edge of the ring band. This value is expressed in part program units and must be greater than or equal to zero (a value of zero means an inner edge of the ring band coincides with the feature nominal.)

Entry Name: RingBand_Inner

Entry Type: Real Number to specify distance in part units. Default value is 0.5.