Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Analog Disk Bottom Hits Distance From Edge

During disk calibration on an analog probe, PC-DMIS measures the bottom of the disk. Defines the distance in millimeters from the outer edge of the bottom of the disk at which PC-DMIS takes hits.

Entry Name: ProbeQualAnalogDiskBottomHitsDistancefromEdge

Entry Type: Real number specifying distance. The default is 2.