Current Help System: PC-DMIS Settings Editor (View Core Help)

### Dim Info (option) Default

These values determine whether the specified option is displayed as part of a Dimension Command. The option is displayed when the value is TRUE (1).

Entry Name: DimInfo(option)Default

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

Options Key:

Auto | Toggles whether PC-DMIS will automatically determine the information that is displayed as part of dimension commands. The following information is displayed when this value is TRUE (1): Measured, Nominal, Tolerances, Deviation, MaxMin, OutTol.
Deviation | Deviation of the measured value from the nominal
GraphOption | Toggles whether a graph will be displayed in the Dimension Info box in the Graphics Display window.
LocA | Location Angle (for cones)
LocD | Location Diameter
LocF | Location Integrated Form Dimension
LocH | Location Height
LocL | Location Length (used for cylinders, slots, cones, and ellipses)
LocPA | Location Polar Angle
LocPD | Location Diameter of a Circle (perpendicular to the pin vector)
LocPR | Location Polar Radius
LocR | Location Radius
LocRS | Location Deviation along a surface report
LocRT | Location Deviation along the Report vector
LocS | Location Deviation along the Surface vector
LocT | Location Error along approach vector (for points on curved surfaces)
LocUseDimAxes | Uses the axes that were previously defined in the dimension's dialog box for Location Dimensions
LocV | Location Vector
LocWorst | Uses the axis that gives the worst out of tolerance condition for Location Dimensions.
LocX | Location X Axis
LocY | Location Y Axis
LocZ | Location Z Axis

Maxmin | Maximum and minimum values for the dimension
Mean | Average of all the deviations for the dimension
Measured | Actual measured dimensions
Nominal | Theoretical values for the dimension
Numpoints | Number of points used to measure the feature of the dimension
Outtol | Out of tolerance measured value from the nominal and tolerance values
ShowDimID | Toggles the ability to display the ID for the dimension within the Graphics Display window
ShowFeatID | Toggles the ability to display the ID for the feature whose dimensions are being measured
ShowHeadingsID | Toggles the display of row and column headings in the Dimension Info box
Stddev | Standard deviation of all the deviations for the dimension
Tolerance | Acceptable tolerance levels either greater than or less than the nominal
TPD1 | True Position diameter/width value of the first datum
TPD2 | True Position diameter/width value of the second datum
TPD3 | True Position diameter/width value of the third datum
TPDF | True Position diameter of Feature
TPForm | True Position integrated form dimension for the feature
TPPA | True Position polar angle
TPPR | True Position polar radius
TPTP | True Position Tolerance
TPUseDimAxes | Uses the axes that were previously defined in the dimension's dialog box for True Position
TPWorst | Uses the axis that gives the worst out of tolerance condition for True Position
TPX | True Position X Axis
TPY | True Position Y Axis
TPZ | True Position Z Axis