Current Help System: PC-DMIS Settings Editor (View Core Help)

### Iterate And RePierce Cad On Best Fit Alignments Tolerance In MM

This value is used in conjunction with the "IterateAndRePierceCadOnBestFitAlignments" when that value is set to TRUE. The find nominals Tolerance is used during the alignment fitting process. This value must be larger than the Probe radius value. The default value should be sufficient in most cases.

Entry Name: IterateAndRePierceCadOnBestFitAlignmentsToleranceInMM

Entry Type: Real Number specifying the Tolerance in mm. Default value is 20.