Current Help System: Tutor Translator (View Core Help)

### Circle Measurement Commands

MCIR(MEMORY[10],4,1) translates to è

ASSIGN/E.BADMEAS=0
RECALL/ALIGNMENT,INTERNAL,E.ALIGNMENTS [1]

CIR2 =FEAT/CIRCLE,RECT,OUT,LEAST_SQR

THEO/<0,0,0>,<0,0,1>,1,0
ACTL/<0,0,0>,<0,0,1>,1,0
MEAS/CIRCLE,4,WORKPLANE
…
… move/hit/tip commands
…
ENDMEAS/

RECALL/ALIGNMENT, INTERNAL, E.ALIGNMENTS [E.CUR_ALIGN]
ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("CIR2")
ASSIGN/E.MEMORY[10]=E.WM1
…
… Evaluation commands.
…

MCIR(4,C3D) translates to è

ASSIGN/E.BADMEAS=0

CIR3 =FEAT/CIRCLE,RECT,IN,LEAST_SQR

THEO/<0,0,0>,<0,0,1>,1,0
ACTL/<0,0,0>,<0,0,1>,1,0
MEAS/CIRCLE,4,3D
…
… move/hit/tip commands
…
ENDMEAS/

ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("CIR3")
…
… Evaluation commands.
…

MCIR(ELEVAR,4) CMIN translates to è

ASSIGN/E.BADMEAS=0

CIR4 =FEAT/CIRCLE,RECT,IN,MIN_CIRCSC

THEO/<-0.098,0.0006,-9.9995>,<0.0099995,0,0.99995>,10.31,0
ACTL/<-0.098,0.0006,-9.9995>,<0.0099995,0,0.99995>,10.31,0
MEAS/CIRCLE,3,WORKPLANE
…
… move/hit/tip commands
…
ENDMEAS/

ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT ("CIR4")
ASSIGN/ELEVAR = E.WM1
…
… Evaluation commands.
…

MCIR(4) CMAX translates to è

ASSIGN/E.BADMEAS=0

CIR4 =FEAT/CIRCLE,RECT,IN,MAX_INSC

THEO/<-0.098,0.0006,-9.9995>,<0.0099995,0,0.99995>,10.31,0
ACTL/<-0.098,0.0006,-9.9995>,<0.0099995,0,0.99995>,10.31,0
MEAS/CIRCLE,3,WORKPLANE
…
… move/hit/tip commands
…
ENDMEAS/

ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("CIR4")
…
… Evaluation commands.
…

MCIR (MEMORY [10], 3) DM 12.93 translates to è

ASSIGN/E.BADMEAS=0

CIR5 = FEAT/CIRCLE,RECT,IN,FIXED_RAD

THEO/<0.002,0.0006,10>,<0.0099995,0,0.99995>,12.93,0
ACTL/<0.002,0.0006,10>,<0.0099995,0,0.99995>,12.93,0
MEAS/CIRCLE,3,WORKPLANE
…
… move/hit/tip commands
…
ENDMEAS/

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT ("CIR5")
ASSIGN/E.MEMORY [10] = E.WM1
…
… Evaluation commands.
…

More:

Not Aligned Circle