Current Help System: Tutor Translator (View Core Help)

### Sphere Measurement Commands

The following commands that use ISO algorithm dont have an equivalent PC-DMIS command. See the section on r;Measurement Commands with no PC-DMIS Equivalent for more information.

MSPH (MEMORY [10], 6)
MSPH (MEMORY [10], 6, FORM ISO) translates to θ

ASSIGN/E.BADMEAS=0

SPH1 = FEAT/SPHERE,RECT,IN

THEO/<10,20,30>,<0,0,1>,23
ACTL/<10,20,30>,<0,0,1>,23
MEAS/SPHERE,5
move/hit/tip commands
ENDMEAS/

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("SPH1")
ASSIGN/E.MEMORY[10] = E.WM1
Evaluation commands.