Current Help System: Tutor Translator (View Core Help)

#### PC-DMIS

1. Theoretical Probe definition.

2. Movement and measured coordinates are computed taking care of all probe parameters.

3. Meaningful Probe Name.

4. Encapsulated Calibration/Qualification.

5. Probes file management command allows only Loading.

The adopted solution is to avoid Calibration and Qualification translation. The user is invited to use PC-DMIS probe management to create a probe file for all required probes. To relate Tutor with PC-DMIS probes the user must create a map file (.T2P = Tutor to PC-DMIS). Each line of this file contains Tutor Head and Tip number and the PC-DMIS probe name.

Because Tutor allows variables to be used for probe selection the translator creates a 2D array loaded with PC-DMIS probe names.