Current Help System: Tutor Translator (View Core Help)

## Element Comment

This command is normally placed before measure, construction, relation, tolerance and define element commands. With PC-DMIS this comment is stored in the TutorElement using the new COMMENT field. It is necessary to store the comment after the TutorElement creation.

MEMORY[2]="This is the second point" MSH(MEMORY[2],1) path PT2 translates to ่

ASSIGN/E.BADMEAS=0

PNT1 = FEAT/POINT,RECT

ENDMEAS/

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PNT1")
ASSIGN/E.WM1.COMMENT = r;This is the second point
ASSIGN/E.MEMORY[2] = E.WM1
Evaluation commands.

In case a string variable is in the place of an immediate string the command is:

WM1=STRVAR translates to ่

ASSIGN/E.WM1=E.STRVAR