Current Help System: Tutor Translator (View Core Help)

### Sphere Construction Commands

The following commands that use ISO algorithm dont have an equivalent PC-DMIS command. See the section on r;Construction Commands with no PC-DMIS Equivalent for more information.

ISPH (MEMORY[10],5, MEMORY[101])
ISPH (MEMORY[10],5, MEMORY[101],FORM LSM)
ISPH (MEMORY[10],5, MEMORY[101],FORM ISO) translates to θ

Warning Messages for FORM ISO

SPH1 =FEAT/SPHERE,RECT,OUT

THEO/<10,20,30>,<0,0,1>,22.9999
ACTL/<10,20,30>,<0,0,1>,22.9999
CONSTR/SPHERE,BF,E.MEMORY[101].ID,E.MEMORY[102].ID,E.MEMORY[103].ID,
E.MEMORY[104].ID,E.MEMORY[105].ID,,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("SPH1")
ASSIGN/E.MEMORY[10] = E.WM1
Evaluation commands.

ISPH (MEMORY[11], MEMORY[103], MEMORY[101], MEMORY[105], MEMORY[102], MEMORY[104])
ISPH (MEMORY[11], MEMORY[103], MEMORY[101], MEMORY[105], MEMORY[102], MEMORY[104], FORM LSM)
ISPH (MEMORY[11], MEMORY[103], MEMORY[101], MEMORY[105], MEMORY[102], MEMORY[104] ,FORM ISO) translates to θ

Warning Messages for FORM ISO

SPH2 =FEAT/SPHERE,RECT,OUT

THEO/<0,20,30>,<0,0,1>,22.9999
ACTL/<10,20,30>,<0,0,1>,22.9999
CONSTR/SPHERE,BF,E.MEMORY[103].ID,E.MEMORY[101].ID,E.MEMORY[105].ID,
E.MEMORY[102].ID,E.MEMORY[104].ID,,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("SPH2")
ASSIGN/E.MEMORY[11] = E.WM1
Evaluation commands.