Current Help System: Tutor Translator (View Core Help)

### Line Construction Commands

The command ILINE is translated with the equivalent PC-DMIS command:

LIN2 =FEAT/LINE,RECT,UNBND

THEO/<xxx,yyy,zzz>,<i,j,k>
ACTL/<1,0,-9.9995>,<0,0,1>
CONSTR/LINE,BF, RefType,E.MEMORY[103].ID,E.MEMORY[106].ID,,

Legend:
xxx = X coordinate | I = vector x component
yyy = Y coordinate | J = vector y component
zzz = Z coordinate | K = vector z component

The refType field is:

- 2D if the L2D Tutor keyword is specified.

- 3D if the L2D Tutor keyword is not specified.

The commands that use FORM ISO algorithm actually dont have equivalent commands on PC-DMIS. See the section on r;Construction Commands with no PC-DMIS Equivalent for more information.

ILINE (MEMORY[36], 2, MEMORY[101]) translates to θ

LIN1 =FEAT/LINE,RECT,UNBND

THEO/<152.003,236.002,151.514>,<-0.0000167,-0.9837928,-0.1793088>
ACTL/<152.003,236.002,150.003>,<-0.0000254,-0.9964263,-0.0844669>
CONSTR/LINE,BF,3D,E.MEMORY[101].ID,E.MEMORY[102].ID,,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("LIN1")
ASSIGN/E.MEMORY[36] = E.WM1
Evaluation commands.

ILINE (MEMORY [37], MEMORY[103],MEMORY[104]) translates to θ

LIN2 =FEAT/LINE,RECT,UNBND

THEO/<152.002,96.001,120.001>,<-0.0000062,0.999924,-0.0123324>
ACTL/<152.004,96.001,130.001>,<-0.0000062,0.999924,-0.0123324>
CONSTR/LINE,BF,3D,E.MEMORY[103].ID,E.MEMORY[106].ID,,

ASSIGN/E.WM1 = TUTORELEMENT("LIN2")
ASSIGN/E.MEMORY[37] = E.WM1
Evaluation commands.

ILINE (MEMORY [38], 2, MEMORY [101], L2D) translates to θ

LIN3 =FEAT/LINE,RECT,UNBND

THEO/<152.003,236.002,151.514>,<0,-1,0>
ACTL/<152.003,236.002,151.514>,<0,-1,0>
CONSTR/LINE,BF,2D,E.MEMORY[101].ID,E.MEMORY[102].ID,,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("LIN3")
ASSIGN/E.MEMORY[38] = E.WM1
Evaluation commands.

ILINE (MEMORY[39],memory[103],memory[106],L2D) translates to θ

LIN4 =FEAT/LINE,RECT,UNBND

THEO/<152.004,-96.0004,131.515>,<0,0.999924,-0.0123318>
ACTL/<152.004,-96.0004,131.515>,<0,0.999924,-0.0123318>
CONSTR/LINE,BF,2D,E.MEMORY[103].ID,

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("LIN4")
ASSIGN/E.MEMORY[39] = E.WM1
Evaluation commands.

The following commands that use ISO algorithm dont have an equivalent PC-DMIS command. See the section on r;Construction Commands with no PC-DMIS Equivalent for more information.

ILINE (MEMORY [22], 2, MEMORY[101] ,FORM ISO)
ILINE (MEMORY [23], MEMORY[102],MEMORY[105], FORM ISO)
ILINE (MEMORY [24], 2, MEMORY[101], L2D ,FORM ISO)
ILINE (MEMORY [24], MEMORY[102],MEMORY[105], L2D, FORM ISO)