Current Help System: Tutor Translator (View Core Help)

### Torus Measurement Commands

PC-DMIS does not have MTORUS equivalent for either measurement or construction commands. See the section on ”r;Measurement Commands with no PC-DMIS Equivalent” for more information.

MTORUS (MEMORY[100],12) translates to è

…
… Warning message
…
ASSIGN/E.BADMEAS=0

SCN1 = FEAT/SET,RECT

THEO/<152.0023,176.6688,118.5883>,<0,0,1>
ACTL/<152.0023,176.6688,118.5883>,<0,0,1>
MEAS/SET,6
MOVE/POINT,<152.003,236.002,130.003>
HIT/BASIC,<152.003,236.002,151.514>,<152.003,236.002,151.514>,USE THEO = NO
…
… other move/hit/tip commands.
…
ENDMEAS/

ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("SCN1")
ASSIGN/E.MEMORY[3]= E.WM1
…
… Evaluation commands.
…