Current Help System: Tutor Translator (View Core Help)

#### Perpendicularity

PERPEN(MEMORY[120], MEMORY[123]) translates to è

DIM PERP1= PERPENDICULARITY OF LINE E.MEMORY[120].ID,RFS TO CYLINDER E.MEMORY[123].ID,RFS EXTENDLENGTH=0.0000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 .0100 0.0000 10.0000 5.0000 5.0000 10.0000 9.9900 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[120].TP = PERP1.MEAS
ASSIGN/E.MEMORY[120].GTOL = 3
ASSIGN/E.WM1 = E.MEMORY[120]

PERPEN(>MEMORY[130], MEMORY[120], MEMORY[123]) translates to è

DIM PERP2= PERPENDICULARITY OF LINE E.MEMORY[120].ID,RFS TO CYLINDER E.MEMORY[123].ID,RFS EXTENDLENGTH=0.0000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 .0100 0.0000 10.0000 5.0000 5.0000 10.0000 9.9900 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = E.MEMORY[120]
ASSIGN/E.WM1.TP = PERP2.MEAS
ASSIGN/E.WM1.GTOL = 3
ASSIGN/E.MEMORY[130] = E.WM1

PERPEN DIST(MEMORY[120], MEMORY[123],6.) translates to è

DIM PERP3= PERPENDICULARITY OF LINE E.MEMORY[120].ID,RFS TO CYLINDER E.MEMORY[123].ID,RFS EXTENDLENGTH=12.0000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 8.4853 4.2426 4.2426 8.4853 8.4753 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[120].TP = PERP3.MEAS
ASSIGN/E.MEMORY[120].GTOL = 3
ASSIGN/E.WM1 = E.MEMORY[120]

PERPEN DIST(MEMORY[120], MEMORY[123], DISTVAR) translates to è

Where the variable DISTVAR contains the dist value.

DIM PERP5= PERPENDICULARITY OF LINE E.MEMORY[120].ID,RFS TO CYLINDER E.MEMORY[123].ID,RFS EXTENDLENGTH=DISTVAR*2 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 8.4853 4.2426 4.2426 8.4853 8.4753 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[120].TP = PERP5.MEAS
ASSIGN/E.MEMORY[120].GTOL = 3
ASSIGN/E.WM1 = E.MEMORY[120]

Warning: For commands where the checked element is a plane, the datum element is a line and the DIST is required the following comment is written in place of the tolerance:

COMMENT/DOC,=====================================
,WARNING: PERPENDICULARITY BETWEEN PLANE AND
,LINE USING PROJECTION, DISTANCE IS NOT ALLOWED
,==================================================