Current Help System: Tutor Translator (View Core Help)

### Output Basics

HEADER(”r;C:\WTutor\header.txt”) translates to è

=CALLSUB/TUTOR_HEADER,TutorSub.PRG:E.OFMT,"C:\WTutor\header.txt ",,

HEADER(”r;This is an Header String”) translates to è

=CALLSUB/TUTOR_HEADER,TutorSub.PRG: E.OFMT,"This is an Header String ",,
HEADERFILE = ”r;C:\WTutor\header.txt”

HEADER(HEADERFILE) translates to è

ASSIGN/HEADERFILE = "C:\WTutor\header.txt"
=CALLSUB/TUTOR_HEADER,TutorSub.PRG: E.OFMT, HEADERFILE,,
HEADERSTR = ”r;This is an Header String”

HEADER(HEADERSTR) translates to è

ASSIGN/HEADERSTR = "This is an header string"
=CALLSUB/TUTOR_HEADER,TutorSub.PRG: E.OFMT, HEADERSTR,,

OUTPUT ON translates to è

ASSIGN/ E.OFMT.ON=1

OUTPUT OFF translates to è

ASSIGN/ E.OFMT.ON=0

OUTPUT MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",,,

OUTPUT DY MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",2,,

OUTPUT PRN MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",3,,

OUTPUT FILE1 MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",4,,

OUTPUT FILE2 MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",5,,

OUTPUT FILE3 MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",6,,

OUTPUT FILE4 MEMORY[10] translates to è

=CALLSUB/TUTOR_OUTPUT,TutorSub.PRG:E.MEMORY[10], E.OFMT, E.TH,"MEMORY[10]",7,,

The following two commands use a string variable for the STR_VAR value:

OUTPUT STR_VAR translates to è

=CALLSUB/TUTOR_OUTSTRING,TutorSub.PRG: E.OFMT,1, E.STR_VAR,,

OUTPUT ("THIS IS AN OUTPUT STING") translates to è

=CALLSUB/TUTOR_OUTSTRING,TutorSub.PRG: E.OFMT,1, "THIS IS AN OUTPUT STING",,

The following Tutor output commands are not translated:
OUTPUT SLINE(1, 2, 3 of 4) MEMORY[10]
COMPARE
OUT_GRAPH
SYNCHRODEV or NO_SYNCHRODEV (PD-DMIS is always synchronized)