#### Measure a Plane

Red Dots show Possible Hit Locations on the Part's Surface

Verify that PC-DMIS is set to Program mode before taking hits. Select the Program mode icon to do this. | Take three hits on the top surface. The hits should be triangular in shape and as spread out as possible. Press the END key after the third hit. PC-DMIS will display a feature ID and a triangle, indicating the measurement of the plane.

Hint: As you take hits, PC-DMIS stores them inside of a hit buffer. If you take a bad hit, you can delete it from the hit buffer by pressing ALT + - (minus) on your keyboard and retake the hit. When you are ready, press END to complete the feature measurement.