#### Center Basic Scan - Key In Method

This method lets you type the X, Y and Z values of the start and end points for the Center scan.

1. Double-click the desired point in the List in the ‘#’ column. This will display an Edit Scan Item dialog box:

Edit Scan Item dialog box

2. Manually edit the X, Y, or Z value.

3. Press the OK button to apply the changes.

The Cancel button will disregard any changes that have been made and will close the dialog box.

You should also key in the CutVec and the InitVec of the center using this same process.