### Measure All

Similar to Measure Marked, the Measure All button also opens the Execution Mode Options dialog box.

- If you are using Measure 3 Spheres, Measure 3 Point Sets, or Measure 3 Points, then this dialog box will first prompt you to measure the three features before prompting you to move the CMM. After moving the machine, you will be prompted to re-measure the same features in the same order.

- If you are using Measure Datums, then the Execution Mode Options dialog box prompts you to measure all the datum features once you have moved the CMM, not before.

The results box will display the 3D distance between the features taken before the move and after the move of the CMM. If you find the results unsatisfactory then you may re-measure the last set of features again as the button will now read: Re-measure.

Note: If the re-measure process proves unsatisfactory, then you must reset the leapfrog and start again from the beginning. This is a problem with all leapfrog systems and should be remembered.