### Jump

The Jump button automatically stops execution (if you're using a DCC machine) and displays the Jump to Feature List dialog box. From this list, you can select the next feature to execute, thereby deviating as needed from the automatically generated execution path.

Jump to Feature List dialog box

After you select a feature from the list, click OK, and PC-DMIS will execute the selected feature. After it finishes, it will return to the pre-defined path and attempt to execute the next non-measured feature until you click Jump again and select a new feature.

Example:

Suppose you have seven circles, labeled CIR1 through CIR7 and they are programmed to execute in that order. If after CIR1, you click Jump and select CIR6, PC-DMIS will immediately measure CIR6. When finished, it will return and measure circles CIR2 through CIR5, and then it will finish by measuring CIR7.