#### Default Feature Tolerance

Default Feature Tolerance area

The Default Feature Tolerance area, enabled when you select the Feature Type option from the Apply Defaults Based On area, lets you define default dimension tolerances based on individual feature types.

Note: This capability only applies for legacy dimensions.

Whenever you manually create a location dimension or whenever PC-DMIS creates any dimension automatically (due to the Auto Dimension Setup... button), the default dimension tolerance associated with that feature type will be used, unless that same feature type already exists in the part program. In that case, PC-DMIS will instead use the tolerance for the existing feature for any new automatic dimensions of that same feature type. This way you only need to modify the tolerance once for a feature type and PC-DMIS will use that same tolerance for other features of the same type throughout the rest of your part program.

Item | Description
Type list | This list displays all the features for which you can set a default tolerance.
Tolerance box | This box defines the default tolerance used for the feature in the Type list.
Apply All button | This button lets you apply the current tolerance value in the Tolerance box to all feature types.

Modified in v44 per PR 256827.