#### Retract Distance

The Retract Distance box lets you enter the distance the probe retracts from the surface after taking a hit. If necessary, it can be automatically changed by PC-DMIS when taking hits on an arc or circle.

The Edit window command line for this option reads:
RETRACT/ nnn.nnnn

Note: Some controllers do not retract on their own. In these cases, PC-DMIS issues the move to do the retract, and the distance is based on ball surface to the part's theoretical hit location. If the controller does do the retract, the distance may be calculated either from the ball surface or the ball center to either the theoretical or measured hit location, depending on the particular controller.