#### Importing Markings for Feature Based Measurements

PC-DMIS's Feature Based Measurement (FBM) functionality is only available if your portlock is programmed with the Feature Based Measurement module.

The Edit | Markings | Import Feature Based Measurement menu item imports a previously exported XML file that contains marking information of specific features. When you import the desired XML file, PC-DMIS automatically marks the specified commands. The XML file must be in the format required by Feature Based Measurement. For more information, see Using Feature Based Measurement.