## Setting Probe Depth

To program measurements off-line, it is important to set the depth of the probe at a specified distance (in relation to the surface of the current working plane). PC-DMIS offers several methods for setting the probe’s depth.

Note: It is necessary to be in Program mode to use any of these techniques. Verify that the STATE button displays PROG.

More:

Setting Approximate Probe Depth

Setting Probe Depth on a Feature

Setting Probe Depth on a Sphere

Setting Probe Depth on a Cone

Keying in Probe Depth