#### Create Analysis View Command

The Analysis window's Options | Create Analysis View Command menu option displays the ANALYSISVIEW command in the Edit window. When this command is marked and executed, PC-DMIS will display the list of dimensions in its own analysis level window, with the number of view and rotations selected previously. It will automatically take a screen capture of the Analysis Level window with the listed dimensions. These screen captures are then available to be displayed and printed in the inspection report.

The Edit window command line for this option reads:
ANALYSISVIEW/D1,D2,D3,,

D1,D2,D3 = list of dimensions to be displayed.

There is no limit to the number of dimension parameters that can be used.

Typing "ANALYSISVIEW" in the Edit window also creates an ANALYSISVIEW command. Any dimensions selected for analysis will become parameters for this command.