### Max / Min Boxes

Available to Linear Open, Linear Close, Patch, and Section scans

The Max / Min increment and angle boxes described below are available when using the VARIABLE scanning technique described in the "Direction 1 Technique (Variable Method)" topic. Only the Max Incr box is available for all the scanning techniques.

Max Increment

The Max Incr box allows you to set the maximum increment distance. Even though increments may increase while using the Variable option, the increments will never be greater than this distance.

Min Increment

The Min Incr box allows you to set the minimum increment. Even though increments may decrease using the Variable option, the increments will never be smaller than this distance.

Max Angle

The Max Ang box allows you to set the maximum angle. Even though angles measured may increase while using the Variable option, the angles will never be greater than this value.

Min Angle

The Min Ang box allows you to set the minimum angle. Even though angles measured may decrease while using the Variable option, the angles will never be less than this value.