### Parameter Settings: I/O Channels tab

Parameter Settings dialog box-I/O Channels tab

Currently, the options on the I/O Channels tab only function on DEA machines. Other machine types may be added in the future. | With the I/O Channels tab, you can select options related to the use of controller I/O channels and place an IOCHANNEL/ command into the Edit window that will define the state of the controller.

Some machine controllers are equipped with I/O channels that can be SET to an ON state (a value of 1) or RESET to an OFF state (a value of 0). The IOCHANNEL/ command tells PC-DMIS to set the state as specified.

To edit information in the I/O Channels tab:

1. Access the Parameter Settings dialog box (Edit | Preferences | Parameters).

2. Click on the I/O Channels tab.

3. Make any changes.

4. Click Apply or OK.

More:

Channel

Set and Reset Options