#### Auto Plane Paths

PC-DMIS provides two different paths for a plane. It automatically chooses the appropriate path based on the diameter and the size of the usable portion of the laser stripe. For auto planes, PC-DMIS always scans perpendicular to the direction of the stripe.

Path 1: Smaller Width

Planes with a width smaller than the usable portion of the stripe

Path 2: Larger Width

Planes with a width larger than the usable portion of the stripe