### Laser Plane

Plane Auto Feature

To create an auto plane using a laser probe:

1. Access the Auto Features dialog box, and select Plane.

2. Do one of the following:

1. Click on time on the cad to give the plane a location and vector. Then manually enter any remaining information.

2. Move the machine to the center of the plane using the Laser View tab of the Graphics Display Window. Next Click the Read Point from Position button. Then manually enter the any remaining information like the display, width, length, etc.

3. Manually enter all of the theoretical x, y, z, i, j, k, display, width, length, etc.

3. Enter the necessary information in the Probe Toolbox tabs. You will likely want to cycle through the Laser Scan, Laser Filtering, and Laser Clipping, properties tabs to enter the information.

4. Click the Test button if desired. Warning: The machine will now move!

5. Click the Create button and then Close.

More:

Plane Specific Parameters

Plane Command Mode Text

Auto Plane Paths