IMPORT – This command imports a statistical value from the data currently being monitored. The current database and filter are used. The format is:

IMPORT Variable=PartName:VariableName:StatVar;

- Variable is the name of a variable created using the DECLARE command.

- PartName is any of the part names in the Part List of monitor mode.

- VariableName is any variable that appears in the Variable List of monitor mode of the specified PartName.

- StatVar is any of the supported statistical calculations. Currently the stats supported for this command are:

MEA (mean)
STD (standard deviation)
MAX (maximum value)
MIN (minimum value)
RNG (range)
NOM (nominal value)
DEV (average deviation)
NUM (number of measurements)
LST (value of last measurement)

an example:

IMPORT CIR1DLAST=DEMO:CIR1.D:LST;