### Importing an XYZIJK File into an Inspection Plan

To import an XYZIJK file into an inspection plan:

1. From the Plan window, select the plan into which you want to import the features.

2. Select the File | Import | XYZ into Plan... menu option. An Open dialog box appears.

3. Navigate to the directory containing the file to import.

4. Click Open when ready to import the file. Planner interprets and imports the selected XYZIJK file into the selected plan.

5. Planner displays the features added to the plan in the XYZ File dialog box.

Note: While this procedure deals specifically with importing XYZIJK features into the inspection plan, the information on XYZIJK files discussed in the "Importing an XYZIJK File into CAD" topic is applicable here as well.