### Use Special Learnmode Probe Parameter Handling

This option provides probe parameter handling during learnmode. It compensates for errors that might occur in part programs that have different probe types that are managed differently by controllers. For example, an analog and trigger probe in the same part program used to return errors from the controller depending on the location of your cursor in the Edit Window. This option is used when set to TRUE (1).

Entry Name: UseSpecialLearnmodeProbeParameterHandling

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 1 unless you are using a portable machine, where the default value is 0.