### Use Point Method Find Hole

This entry lets you specify whether or not PC-DMIS uses sample hits to measure a newly found hole. If you set this entry to TRUE (1), then holes will be measured as they were in PC-DMIS version 2.3, without using sample hits. If you set this entry to FALSE (0), then holes are measured using sample hits.

Entry Name: UsePointMethodFindHole

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.