### DCC IJK (1-4)_0

Provides the default "I" value for various IJK vectors that are used in the creation of Auto Features. The value is applied to different vector types (Surface, Edge, Angle, etc.) depending on the auto feature type.

Note: Because of the variance between auto features and how this value is applied, it is best to alter this value from the Auto Feature dialog box within PC-DMIS.

Entry Name: DccIJK(1-4)_0

Entry Type: Real Number to specify the I vector value. Default value is 0.