### Probe Use Trax Algorithm

When calibrating an analog probe on some machine types, particularly when using the Leitz interface, there is typically a choice of whether or not to use the TRAX calibration algorithm for calculating the calibration coefficients.

This value stores the last used value for the checkbox in the Probe Utilities dialog box. When this value is set to TRUE (1), the TRAX algorithm is used.

Entry Name: ProbeUseTraxAlgorithm

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). The default is 0.