## Auto Insert Moves

The registry values in this section are used in conjunction with the PC-DMIS capability to Automatically Insert Clearance Moves within PC-DMIS Inspection Planner. The following options provide the criteria for how clearance moves are added to your imported Inspection Plan:

More:

BelowTriggerTolerancePercentage

CollisionMoveClearanceInMM

CollisionTolleranceinMM

ConeAngleForMoveOverPath

DeleteMovesBeforeInsert

SmallestTipSearchIncrementInDegrees