### Multi Sec Scan Type

Determines the section type for Multisection Manual scan.

Entry Name: MultiSecScanType

Entry Type: Whole Number specifying section type number. Default value is 0.

Section Type Key

0 | Parallel Planes | The sections are planes running through your part. Every time the probe crosses a plane, PC-DMIS records a hit. Planes are relative to the start point and direction vector.
1 | Radial Planes | These sections are planes radiate out from the start point. Every time the probe crosses a plane, PC-DMIS takes a hit.
2 | Concentric Circles | These sections are concentric circles with increasingly larger diameters centered around the start point. Every time the probe crosses a circle, PC-DMIS takes a hit.