### DCC Edge Point 2 Click Select Show Warning

This entry allows you to specify whether or not PC-DMIS shows a warning alerting you that PC-DMIS expects two mouse clicks (one on each surface) for creating auto edge points. If this entry and the DCCEdgePoint2ClickSelect entry are both set to TRUE, PC-DMIS displays a message informing you that you will need to take two mouse clicks to create the auto edge point.

Entry Name: DCCEdgePoint2ClickSelectShowWarning

Entry Type: True/False value. Default value is TRUE.

See "DCC Edge Point 2 Click Select".

For information on Auto Edge Points, see the "Creating an Auto Edge Point" topic in the "Creating Auto Features" chapter.